# 4-8 Ferndell St SOUTH GRANVILLE NSW 2142

PO Box 3107 WETHERILL PARK NSW 2164

Ph: (02) 9632-5000

Fx: (02) 9632-5011

ABN: 18 165 515 257

**PRODUCT DATA AND APPLICATION SHEET**

**PRODUCT NAME L5 Neutral or Active Link**

**PRODUCT CODE** L5, L5R

**DESCRIPTION** Neutral Link 5 Hole 100amp with Cover

**BOX QUANTITY** 10 **OUTER QUANTITY** 100

# FEATURES

* 5 Hole Neutral Link with two screws per tunnel;
* 3 tunnels, 5.5mm diameter accommodate 1 x 16 sq mm cable;
* 2 tunnels, 8mm diameter accommodate 1 x 25 sq mm cable
* Dimensions: 65 x 46 x 43 mm


# APPLICATIONS

Neutral link 5 hole for service cable switchboards have an outer casing made of a tinted transparent poly-carbonate. The transparent cover enables you to check wiring and locate the sealing screw at a glance. Neutral link 5 pole utilizes a brass bar to link the main to the rest of the circuit. Neutral link 5 pole are ideal for both commercial and industrial use in switchboards as it can take cables of up to 25mm in size. The sealing screw with brass insert, resists stripping.



 *TESLA Electrical Components –Sept17 L5(R)*